3GPP TS 36.213 V15.3.0 (2018-09)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Evolved Universal Terrestrial Radio Access (E-UTRA);

Physical layer procedures

(Release 15)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganisational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organisational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organisational Partners' Publications Offices.

Keywords

E-UTRA, radio, layer 1

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles – Sophia Antipolis

Valbonne – France

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2018, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 8

1 Scope 9

2 References 9

3 Symbols and abbreviations 10

3.1 Symbols 10

3.2 Abbreviations 10

4 Synchronization procedures 12

4.1 Cell search 12

4.2 Timing synchronization 12

4.2.1 Radio link monitoring 12

4.2.2 Inter-cell synchronization 12

4.2.3 Transmission timing adjustments 12

4.3 Timing for Secondary Cell Activation / Deactivation 14

5 Power control 15

5.1 Uplink power control 15

5.1.1 Physical uplink shared channel 15

5.1.1.1 UE behaviour 16

5.1.1.2 Power headroom 30

5.1.2 Physical uplink control channel 33

5.1.2.1 UE behaviour 34

5.1.3 Sounding Reference Symbol (SRS) 39

5.1.3.1 UE behaviour 39

5.1.3.2 Power headroom for Type3 report 41

5.1.4 Power allocation for EUTRA dual connectivity 42

5.1.4.1 Dual connectivity power control Mode 1 42

5.1.4.2 Dual connectivity power control Mode 2 50

5.1.5 Power allocation for PUCCH-SCell 54

5.2 Downlink power allocation 55

5.2.1 eNodeB Relative Narrowband TX Power (RNTP) restrictions 57

6 Random access procedure 59

6.1 Physical non-synchronized random access procedure 59

6.1.1 Timing 60

6.2 Random Access Response Grant 61

7 Physical downlink shared channel related procedures 66

7.1 UE procedure for receiving the physical downlink shared channel 67

7.1.1 Single-antenna port scheme 85

7.1.2 Transmit diversity scheme 85

7.1.3 Large delay CDD scheme 85

7.1.4 Closed-loop spatial multiplexing scheme 85

7.1.5 Multi-user MIMO scheme 86

7.1.5A Dual layer scheme 86

7.1.5B Up to 8 layer transmission scheme 86

7.1.6 Resource allocation 86

7.1.6.1 Resource allocation type 0 88

7.1.6.2 Resource allocation type 1 89

7.1.6.3 Resource allocation type 2 90

7.1.6.4 PDSCH starting position 93

7.1.6.4A PDSCH starting position for BL/CE UEs 95

7.1.6.5 Physical Resource Block (PRB) bundling 95

7.1.7 Modulation order and transport block size determination 97

7.1.7.1 Modulation order and redundancy version determination 99

7.1.7.2 Transport block size determination 105

7.1.7.2.1 Transport blocks not mapped to two or more layer spatial multiplexing 109

7.1.7.2.2 Transport blocks mapped to two-layer spatial multiplexing 118

7.1.7.2.3 Transport blocks mapped for DCI Format 1C and DCI Format 6-2 118

7.1.7.2.4 Transport blocks mapped to three-layer spatial multiplexing 119

7.1.7.2.5 Transport blocks mapped to four-layer spatial multiplexing 119

7.1.7.2.6 Transport blocks mapped for BL/CE UEs configured with CEModeB and PDSCH bandwidth up to 1.4MHz 120

7.1.7.2.7 Transport blocks mapped for BL/CE UEs *SystemInformationBlockType1-BR* 121

7.1.7.2.8 Transport blocks mapped for UEs configured with *ce-pdsch-maxBandwidth-config* value of 5 MHz or with *pdsch-MaxBandwidth-SC-MTCH* value of 24 PRBs 121

7.1.7.3 Redundancy Version determination for Format 1C 121

7.1.8 Storing soft channel bits 122

7.1.9 PDSCH resource mapping parameters 122

7.1.10 Antenna ports quasi co-location for PDSCH 124

7.1.11 PDSCH subframe assignment for BL/CE UE 125

7.2 UE procedure for reporting Channel State Information (CSI) 127

7.2.1 Aperiodic CSI Reporting using PUSCH 137

7.2.2 Periodic CSI Reporting using PUCCH 162

7.2.3 Channel Quality Indicator (CQI) definition 202

7.2.4 Precoding Matrix Indicator (PMI) definition 215

7.2.5 Channel-State Information – Reference Signal (CSI-RS) definition 243

7.2.6 Channel-State Information – Interference Measurement (CSI-IM) Resource definition 245

7.2.7 Zero Power CSI-RS Resource definition 245

7.2.8 CSI-RS Activation / Deactivation 245

7.3 UE procedure for reporting HARQ-ACK 246

7.3.1 FDD HARQ-ACK reporting procedure 248

7.3.2 TDD HARQ-ACK reporting procedure 253

7.3.2.1 TDD HARQ-ACK reporting procedure for same UL/DL configuration 253

7.3.2.2 TDD HARQ-ACK reporting procedure for different UL/DL configurations 268

7.3.3 FDD-TDD HARQ-ACK reporting procedure for primary cell frame structure type 1 276

7.3.4 FDD-TDD HARQ-ACK reporting procedure for primary cell frame structure type 2 277

8 Physical uplink shared channel related procedures 279

8.0 UE procedure for transmitting the physical uplink shared channel 279

8.0.1 Single-antenna port scheme 303

8.0.2 Closed-loop spatial multiplexing scheme 303

8.1 Resource allocation for PDCCH/EPDCCH/SPDCCH with uplink DCI format 304

8.1.1 Uplink resource allocation type 0 304

8.1.2 Uplink resource allocation type 1 305

8.1.3 Uplink resource allocation type 2 305

8.1.4 Uplink resource allocation type 3 306

8.1.5 Uplink resource allocation type 4 307

8.1.5.1 UL Resource Block Groups 307

8.1.6 Uplink resource allocation type 5 308

8.2 UE sounding procedure 310

8.3 UE HARQ-ACK procedure 321

8.3A Autonomous uplink feedback procedure 323

8.4 UE PUSCH hopping procedure 323

8.4.1 Type 1 PUSCH hopping 324

8.4.2 Type 2 PUSCH hopping 324

8.5 UE Reference Symbol (RS) procedure 325

8.6 Modulation order, redundancy version and transport block size determination 326

8.6.1 Modulation order and redundancy version determination 326

8.6.2 Transport block size determination 334

8.6.3 Control information MCS offset determination 340

8.7 UE transmit antenna selection 344

8.8 Transmission timing adjustments 344

9 Physical downlink control channel procedures 344

9.1 UE procedure for determining physical downlink control channel assignment 345

9.1.1 PDCCH assignment procedure 345

9.1.2 PHICH assignment procedure 349

9.1.3 Control Format Indicator (CFI) assignment procedure 352

9.1.4 EPDCCH assignment procedure 353

9.1.4.1 EPDCCH starting position 360

9.1.4.2 Antenna ports quasi co-location for EPDCCH 360

9.1.4.3 Resource mapping parameters for EPDCCH 361

9.1.4.4 PRB-pair indication for EPDCCH 361

9.1.5 MPDCCH assignment procedure 362

9.1.5.1 MPDCCH starting position 368

9.1.5.2 Antenna ports quasi co-location for MPDCCH 369

9.1.6 SPDCCH assignment procedure 369

9.1.6.1 Resource mapping parameters for SPDCCH 370

9.1.6.2 PRB-pair indication for SPDCCH 370

9.1.6.3 Physical Resource Block (PRB) bundling for DMRS-based SPDCCH 371

9.1.6.4 Antenna ports quasi co-location for DMRS-based SPDCCH 371

9.2 PDCCH/EPDCCH/MPDCCH/SPDCCH validation for semi-persistent scheduling 373

9.2A PDCCH/EPDCCH validation for autonomous uplink transmissions 375

9.3 PDCCH/EPDCCH/MPDCCH/SPDCCH control information procedure 376

10 Physical uplink control channel procedures 377

10.1 UE procedure for determining physical uplink control channel assignment 378

10.1.1 PUCCH format information 383

10.1.2 FDD HARQ-ACK feedback procedures 389

10.1.2.1 FDD HARQ-ACK procedure for one configured serving cell 389

10.1.2.2 FDD HARQ-ACK procedures for more than one configured serving cell 393

10.1.2.2.1 PUCCH format 1b with channel selection HARQ-ACK procedure 393

10.1.2.2.2 PUCCH format 3 HARQ-ACK procedure 397

10.1.2.2.3 PUCCH format 4 HARQ-ACK procedure 399

10.1.2.2.4 PUCCH format 5 HARQ-ACK procedure 402

10.1.3 TDD HARQ-ACK feedback procedures 403

10.1.3.1 TDD HARQ-ACK procedure for one configured serving cell 405

10.1.3.2 TDD HARQ-ACK procedure for more than one configured serving cell 419

10.1.3.2.1 PUCCH format 1b with channel selection HARQ-ACK procedure 419

10.1.3.2.2 PUCCH format 3 HARQ-ACK procedure 435

10.1.3.2.3 PUCCH format 4 HARQ-ACK procedure 442

10.1.3.2.4 PUCCH format 5 HARQ-ACK procedure 459

10.1.3A FDD-TDD HARQ-ACK feedback procedures for primary cell frame structure type 2 459

10.1.4 HARQ-ACK Repetition procedure 461

10.1.5 Scheduling Request (SR) procedure 462

10.2 Uplink HARQ-ACK timing 464

11 Physical Multicast Channel (PMCH) related procedures 468

11.1 UE procedure for receiving the PMCH 468

11.2 UE procedure for receiving MCCH and system information change notification 469

12 Assumptions independent of physical channel 469

13 Uplink/Downlink configuration determination procedure for Frame Structure Type 2 469

13.1 UE procedure for determining eIMTA-uplink/downlink configuration 470

13A Subframe configuration for Frame Structure Type 3 471

14 UE procedures related to Sidelink 474

14.1 Physical Sidelink Shared Channel related procedures 475

14.1.1 UE procedure for transmitting the PSSCH 475

14.1.1.1 UE procedure for determining subframes for transmitting PSSCH for sidelink transmission mode 1 477

14.1.1.1.1 Determination of subframe indicator bitmap 477

14.1.1.2 UE procedure for determining resource blocks for transmitting PSSCH for sidelink transmission mode 1 480

14.1.1.2.1 PSSCH resource allocation for sidelink transmission mode 1 480

14.1.1.2.2 PSSCH frequency hopping for sidelink transmission mode 1 481

14.1.1.3 UE procedure for determining subframes for transmitting PSSCH for sidelink transmission mode 2 481

14.1.1.4 UE procedure for determining resource blocks for transmitting PSSCH for sidelink transmission mode 2 482

14.1.1.4A UE procedure for determining subframes and resource blocks for transmitting PSSCH for sidelink transmission mode 3 482

14.1.1.4B UE procedure for determining subframes and resource blocks for transmitting PSSCH and reserving resources for sidelink transmission mode 4 483

14.1.1.4C UE procedure for determining subframes and resource blocks for PSSCH transmission associated with an SCI format 1 483

14.1.1.5 UE procedure for PSSCH power control 485

14.1.1.6 UE procedure for determining the subset of resources to be reported to higher layers in PSSCH resource selection in sidelink transmission mode 4 486

14.1.1.7 Conditions for selecting resources when the number of HARQ transmissions is two in sidelink transmission mode 4 489

14.1.2 UE procedure for receiving the PSSCH 489

14.1.3 UE procedure for determining resource block pool and subframe pool for sidelink transmission mode 2 489

14.1.5 UE procedure for determining resource block pool and subframe pool for sidelink transmission mode 3 and 4 490

14.2 Physical Sidelink Control Channel related procedures 491

14.2.1 UE procedure for transmitting the PSCCH 491

14.2.1.1 UE procedure for determining subframes and resource blocks for transmitting PSCCH for sidelink transmission mode 1 494

14.2.1.2 UE procedure for determining subframes and resource blocks for transmitting PSCCH for sidelink transmission mode 2 495

14.2.1.3 UE procedure for PSCCH power control 495

14.2.2 UE procedure for receiving the PSCCH 496

14.2.3 UE procedure for determining resource block pool and subframe pool for PSCCH 496

14.2.4 UE procedure for determining resource block pool for PSCCH in sidelink transmission mode 3 and 4 497

15 Void 500

16 UE Procedures related to narrowband IoT 501

16.1 Synchronization procedures 501

16.1.1 Cell search 501

16.1.2 Timing synchronization 501

16.2 Power control 501

16.2.1 Uplink power control 501

16.2.1.1 Narrowband physical uplink shared channel 501

16.2.1.1.1 UE behaviour 501

16.2.1.1.2 Power headroom 502

16.2.1.2 SR 502

16.2.1.2.1 UE behaviour 502

16.2.2 Downlink power allocation 503

16.3 Random access procedure 503

16.3.1 Physical non-synchronized random access procedure 503

16.3.2 Timing 504

16.3.3 Narrowband random access response grant 505

16.4 Narrowband physical downlink shared channel related procedures 507

16.4.1 UE procedure for receiving the narrowband physical downlink shared channel 507

16.4.1.1 Single-antenna port scheme 510

16.4.1.2 Transmit diversity scheme 510

16.4.1.3 Resource allocation 510

16.4.1.4 NPDSCH starting position 513

16.4.1.5 Modulation order and transport block size determination 514

16.4.1.5.1 Transport blocks not mapped for *SystemInformationBlockType1-NB* 514

16.4.1.5.2 Transport blocks mapped for *SystemInformationBlockType1-NB* 515

16.4.2 UE procedure for reporting ACK/NACK 515

16.5 Narrowband physical uplink shared channel related procedures 516

16.5.1 UE procedure for transmitting format 1 narrowband physical uplink shared channel 516

16.5.1.1 Resource allocation 518

16.5.1.2 Modulation order, redundancy version and transport block size determination 519

16.5.2 UE procedure for NPUSCH retransmission 521

16.5.3 UE procedure for transmitting SR 521

16.6 Narrowband physical downlink control channel related procedures 521

16.6.1 NPDCCH starting position 526

16.6.2 NPDCCH control information procedure 527

16.6.3 NPDCCH validation for semi-persistent scheduling 527

16.7 Assumptions independent of physical channel related to narrowband IoT 527

16.8 UE procedure for acquiring cell-specific reference signal sequence and raster offset 527

16.9 UE procedure for receiving narrowband wake up signal 528

17 Wake-up signal related procedures for BL/CE UE 529

Annex A (informative): Change history 530